BK-08A

|  |
| --- |
| Product Parameter |
| Dimension | 93x47x38(mm) |
| Glass Thickness | 10-15mm |
| Suitable | Fully Frameless Glass Door |
| Opening Mode | 90 or 180 degree door |
| Use with | BL-C2001 series |
| Weight | 0.15kg |